================================================
v1.0.9
1. Modify for mainline kernel version 5.13.0 or above.
2. Add get/set CAN error function.
3. Remove filter setting and set baud rate of UART function.
4. Re-enable get/set baud rate of CAN and active mode, get all setting, get firmware version and get faro port index functions.
5. Modify note.

================================================
v1.0.8
1. Modify for mainline kernel version 5.4.140

================================================
v1.0.7
1. Fix the socket crashed in kernel version above 5.8.0.

================================================
v1.0.6
1. Modify the driver code to improve performance.
2. Fix the Counting CAN data bug.

================================================
v1.0.5
1. Modify socketCAN driver for kernel version 5.4 or above. 

================================================
v1.0.4
1. Fix receiving bug. If the device gets error data, then set the overrun bit and continue receiving. 

================================================
v1.0.3
1. Make can0 can1 separated.
